USB-8COM(V2) Specifications & Features

- Serial connector: eight DB9 male connecto r
- Power Supply: works in USB self power mode (5V, 500mA), no external power supply is needed
- Adds high speed RS-232 port via USB connection
- 384 byte receive buffer
- 128 byte transmit buffer for high speed data throughput
- Requires no IRQ, DMA, I/O port
- Serial transmission speed up to 921.6 Kbps
- RS-232 data signals : DCD, RxD, TxD, DTR, GND, DSR, RTS, CTS, RI
- Monitor LEDs of TxD, RxD of each port indicating port status
- Virtual COM port drivers available for Windows 7 / Vista / 2003 / XP / 2000